SECTION 00 00 000 – SECTION NAME

1. GENERAL
   * + 1. WARRANTY
          1. Special Warranty:

**EDIT** - Verify

Warranty Period: Years from date of Substantial Completion, for durations indicated.

**EDIT** - Retain applicable subparagraphs below.

The Proximity card readers shall provide a lifetime warranty against defects in materials and workmanship.

1. PRODUCTS
   * + 1. access control reader OPTION – Schlage Open
          1. Manufacturer:

Scheduled Manufacturer: Schlage® SM10, No substitutes will be accepted

Acceptable Substitute: **No Acceptable Substitute**

* + - * 1. Requirements: Read Only Smart Contactless reader

Access control card readers shall be as manufactured by a global company who is a recognized leader in the production of access control devices. Card reader manufactured for non-access control applications shall not be acceptable.

Smart contactless reader shall be NFC-compatible and read access control data from both 125 kHz and 13.56 MHz contactless smart cards. The Smart contactless reader shall be optimally designed for use in access control applications that require reading13.56 MHz contactless smart cards by providing:

Configuration allows reader to be enabled to read smart.

Guaranteed compatibility to read all standard data formats ensuring card-to-reader interoperability in multi-location installations and multi-card/reader populations when used with Schlage products.

Secure access control data exchange between the smart card and the reader utilizing diversified keys and mutual authentication sequences.

Universal compatibility with most access control systems.

Ease of installation through industry standard wiring methods.

Optimal read range and read speed for increased access control throughput.

Global availability.

Product construction suitable for both indoor and outdoor applications.

Customizable behavior for indicator lights and beeper.

Smart contactless reader shall comply with the following 13.56MHz-related standards to ensure product compatibility and predictability of performance:

ISO 14443

Smart contactless reader shall be configurable to read 13.56 MHz data simultaneously from the following cards (multiple credential support based on reader configuration):

Secure support - MIFARE DESFire EV1with PACSA, MIFARE Classic, FIPS 201 PIV Credential.

UID/CSN Support – DESFire Classic V0.06, HID iClass, ISOX (my-d).

Smart contactless reader shall provide the ability to read card access data stored in the secure access control sector/application area of the ISO 14443 XceedID MIFARE or MIFARE DESFire EV1 card.

The Smart contactless reader shall be configurable to provide multiple hierarchical degrees of key compatibility for accessing the smart card access control data. Compatibility shall be provided for the following key structure options:

Compatibility with the default Schlage key structure to ensure convenient off the shelf compatibility with Schlage cards and readers.

Compatibility with custom keys managed by Schlage which provide a site-specific, unique, protected key structure.

Compatibility with high security customer managed custom keys.

Smart contactless reader shall allow the reader firmware to be upgraded in the field without the need to remove the reader from the wall through the use of factory-provided device.

Smart contactless reader shall be suitable for global deployment by meeting worldwide radio and safety regulatory compliance including:

FCC Certification (US)

CE (EU)

C-tick (Australia, New Zealand)

R&TTE Directive (15EU)

UL294 (US)

ULC-S319

IC (Canada)

FIPS201 / PIV I

IP65

Smart contactless reader shall be fully compliant with Restriction of Hazardous Substances directive (RoHS) restricting the use of specific hazardous materials found in electrical and electronic products.

Smart contactless reader shall provide universal compatibility with most access control systems by outputting card data in compliance with the SIA AC-01 Wiegand standard.

Smart contactless reader shall allow for secure installation practices through mounting methods utilizing tamper resistant screws.

Smart contactless reader shall provide the ability to transmit an alarm signal via and integrated optical tamper switch if an attempt is made to remove the reader from the wall. The tamper switch shall be programmable to provide a selectable action to provide a selectable action compatible with various tamper communication schemes provided by access control panel manufacturers. The selectable action shall include one of the following:

The reader open collector line changes from a high state (5V) to a low state (Ground).

If utilizing OSDP Protocol reader shall report a tamper condition via RS485.

Smart contactless reader shall provide the ability for mounting to standard electrical boxes through the use of universal international mounting holes.

Smart contactless reader shall be provided with a full potted assembly.

Smart contactless reader shall be provided with a quick connect wire harness.

The Smart contactless reader shall provide customizable reader behavior options either from the factory, or defined in the field through the use of pre-configured command cards. Reader behavior programming options shall include:

LED & Audio configurations.

Ability to disable reading of specific card technologies or frequencies.

ISO 14443/15693 CSN output configuration.

Wiegand output spacing and timing.

Smart contactless reader shall provide the following programmable audio/visual indication:

An audio beeper shall provide tone sequence to signify: access granted, access denied, power up, and diagnostics.

A light bar shall provide clear visual status (red/green/amber).

Smart contactless reader shall be designed for low current operation to enable migration from most legacy proximity applications without the need to replace existing access control panels and/or power supplies. Contactless smart card power requirements shall be:

Operating voltage: 5 – 16 VDC, reverse voltage protected. Linear power supply recommended.

Current requirements: 65 mA DC, 110 mA PEAK @ 12 VDC

Smart contactless reader shall meet the following physical specifications:

Dimensions: 4.26” x 1.72” x 0.84” (10.8 cm x 4.4 cm x 2.1cm)

Weight: 7.2 oz. (204.16 g)

Material: UL94 Polycarbonate

Plastics: Consist of three-piece design with mounting plate, potted case and aesthetic cover.

Color: Black, Gray, Brown or Cream as approved by the project architect.

Smart contactless reader shall meet the following environmental specifications:

Operating temperature: -31 to 151 degrees F (-35 to 67 degrees C)

Operating humidity: 5% to 95% relative humidity non-condensing

Weatherized design suitable to withstand harsh environments

Certified rating of IP65

Smart contactless reader cabling requirements shall be:

Cable distance: (Wiegand): 500 feet (150m)

Cable type: 5-conductor #22 AWG

Standard reader termination: 18” (0.5m) wire harness

1. EXECUTION

no part 3 INFORMATION IS CONTAINED IN THIS Template.

END OF SECTION

If you require technical specifications or additional information on these products, please visit the Allegion website [here](http://us.allegion.com/en/home/products/categories/readers.html).